Electrocardiogram—electrocardiogram ST-segment-elevation in lead V4R indicator

Exported from METEOR

(AIHW's Metadata Online Registry)

© Australian Institute of Health and Welfare 2024

This product, excluding the AIHW logo, Commonwealth Coat of Arms and any material owned by a third party or protected by a trademark, has been released under a Creative Commons BY 4.0 (CC BY 4.0) licence. Excluded material owned by third parties may include, for example, design and layout, images obtained under licence from third parties and signatures. We have made all reasonable efforts to identify and label material owned by third parties.

You may distribute, remix and build on this website’s material but must attribute the AIHW as the copyright holder, in line with our attribution policy. The full terms and conditions of this licence are available at https://creativecommons.org/licenses/by/4.0/.

Enquiries relating to copyright should be addressed to info@aihw.gov.au.

Enquiries or comments on the METEOR metadata or download should be directed to the METEOR team at meteor@aihw.gov.au.

# Electrocardiogram—electrocardiogram ST-segment-elevation in lead V4R indicator

|  |
| --- |
| Identifying and definitional attributes |
| Metadata item type: | Data Element Concept |
| METEOR identifier: | 343885 |
| Registration status: | [Health!](https://meteor-uat.aihw.gov.au/RegistrationAuthority/14), Standard 01/10/2008 |
| Definition: | An indicator of whether ST-segment-elevation greater than or equal to 1mm (0.1mV) in lead V4R of the electrocardiogram (ECG) is present. |

## Object Class attributes

### Identifying and definitional attributes

|  |  |
| --- | --- |
| Object class: | [Electrocardiogram](https://meteor-uat.aihw.gov.au/content/359999) |
| Definition: | A means of studying the activity of the heart from electrical signals.   |
| Specialisation of: | [Service/care event](https://meteor-uat.aihw.gov.au/content/281121) |

## Property attributes

### Identifying and definitional attributes

|  |  |
| --- | --- |
| Property: | [Electrocardiogram ST-segment-elevation in lead V4R indicator](https://meteor-uat.aihw.gov.au/content/343883) |
| Definition: | Presence of ST-segment-elevation of greater than or equal to 1mm (0.1mV) in lead V4R |
| Property group: | [Physical wellbeing](https://meteor-uat.aihw.gov.au/content/524395) |

## Data element concept attributes

### Relational attributes

|  |  |
| --- | --- |
| Data Elements implementing this Data Element Concept: | [Electrocardiogram—ST-segment-elevation in lead V4R indicator, yes/no code N](https://meteor-uat.aihw.gov.au/content/343889)[Health!](https://meteor-uat.aihw.gov.au/RegistrationAuthority/14), Standard 01/10/2008 |